MOHAMED IRFAN PAKKADA, M Tech, CeNSE.
SR: 05-16-00-10-51-14-1-11296
PROJECT: SIMULATION OF TUNABLE MEMS CAPACITOR USING COMSOL

SOFTWARE: COMSOL MULTIPHYSICS 4.3  
          PHYSICS USED:              
          Electromechanics

          PROCEDURE FOR RUNNING CODE:
          1) Open the file named "sample" in the zip file.
          2) When opened it will show all study and post processing results last executed( by me).
          3) In the left side in 'model builder' expand the model 1, geometry, materials, electromechanics, results etc. to see the construction, specification, and boundary conditions given.
          4) Under 'results', u can see all post processing information.
          5) Whenever the ORIGINAL STRUCTURE want to be seen in the graphics tab(b'z sometime structure is obscure due to bounding to box), use 'wireframe rendering tool'.
          6) To see or change the sweep voltage applied click study1>stationary>study extension.


reference : To modify look at the example given in comsol, model library> mems module> actuators> electrostatically_actuated_cantilever.
       
           